Supplementary information for: *Sodium silicate and hexametaphosphate promote the release of (oxyhydr)oxide nanoparticles from corroding iron*

Benjamin F. Trueman, Javier Locsin, Evelyne Doré, Kalli Hood, and Graham A. Gagnon

Centre for Water Resources Studies,\* Department of Civil & Resource Engineering, Dalhousie University, 1360 Barrington St., Halifax, Nova Scotia, Canada B3H 4R2  
   
 \*Corresponding author  
 E-mail: [benjamin.trueman@dal.ca](mailto:benjamin.trueman@dal.ca)  
 <Tel:902.494.6070>  
 Fax: 902.494.3105

This document contains X tables and X figures.




Figure S1: Fractograms representing pure solutions of sodium hexameta- and trimeta-phosphate.

Table S1. FFF run parameters for globular protein standards.

| Parameter | Value |
| --- | --- |
| Injection volume | 50 µL |
| Spacer | 500 µm |
| Total run time | 33.5 min |
| Detector flow | 1 mL min-1 |
| Injection flow | 0.2 mL min-1 |
| Focus flow | 1.5 mL min-1 |
| Focus period | 5 min |
| Transition period | 1 min |
| Crossflow | 2 mL min-1 |